Initializing cgroup subsys cpuset
Initializing cgroup subsys cpu
Linux version 2.6.25-std-def-alt8.M41.4 (builder@apiary.int.altlinux.org) (gcc version 4.1.2 20070626 (ALT Linux, build 4.1.2-alt2)) #1 SMP Sat Dec 6 14:42:12 MSK 2008
BIOS-provided physical RAM map:
 BIOS-e820: 0000000000000000 - 00000000000a0000 (usable)
 BIOS-e820: 00000000000f0000 - 0000000000100000 (reserved)
 BIOS-e820: 0000000000100000 - 0000000011ef0000 (usable)
 BIOS-e820: 0000000011ef0000 - 0000000011ef3000 (ACPI NVS)
 BIOS-e820: 0000000011ef3000 - 0000000011f00000 (ACPI data)
 BIOS-e820: 00000000fec00000 - 0000000100000000 (reserved)
0MB HIGHMEM available.
286MB LOWMEM available.
Scan SMP from c0000000 for 1024 bytes.
Scan SMP from c009fc00 for 1024 bytes.
Scan SMP from c00f0000 for 65536 bytes.
found SMP MP-table at [c00f4e80] 000f4e80
Entering add_active_range(0, 0, 73456) 0 entries of 256 used
Zone PFN ranges:
  DMA             0 ->     4096
  Normal       4096 ->    73456
  HighMem     73456 ->    73456
Movable zone start PFN for each node
early_node_map[1] active PFN ranges
    0:        0 ->    73456
On node 0 totalpages: 73456
  DMA zone: 32 pages used for memmap
  DMA zone: 0 pages reserved
  DMA zone: 4064 pages, LIFO batch:0
  Normal zone: 541 pages used for memmap
  Normal zone: 68819 pages, LIFO batch:15
  HighMem zone: 0 pages used for memmap
  Movable zone: 0 pages used for memmap
DMI 2.2 present.
ACPI: RSDP 000F6900, 0014 (r0 IntelR)
ACPI: RSDT 11EF3000, 002C (r1 IntelR AWRDACPI 42302E31 AWRD        0)
ACPI: FACP 11EF3040, 0074 (r1 IntelR AWRDACPI 42302E31 AWRD        0)
ACPI: DSDT 11EF30C0, 3D22 (r1 INTELR AWRDACPI     1000 MSFT  100000C)
ACPI: FACS 11EF0000, 0040
ACPI: APIC 11EF6E00, 005C (r1 IntelR AWRDACPI 42302E31 AWRD        0)
ACPI: PM-Timer IO Port: 0x4008
ACPI: Local APIC address 0xfee00000
ACPI: LAPIC (acpi_id[0x00] lapic_id[0x00] enabled)
Processor #0 6:8 APIC version 17
ACPI: LAPIC (acpi_id[0x01] lapic_id[0x01] disabled)
ACPI: IOAPIC (id[0x02] address[0xfec00000] gsi_base[0])
IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-23
ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 high level)
ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
ACPI: IRQ0 used by override.
ACPI: IRQ2 used by override.
ACPI: IRQ9 used by override.
Enabling APIC mode:  Flat.  Using 1 I/O APICs
Using ACPI (MADT) for SMP configuration information
Allocating PCI resources starting at 20000000 (gap: 11f00000:ecd00000)
PM: Registered nosave memory: 00000000000a0000 - 00000000000f0000
PM: Registered nosave memory: 00000000000f0000 - 0000000000100000
Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 72883
Kernel command line: auto BOOT_IMAGE=ALTLinux ro root=UUID=02a1e3ad-17a6-42fd-af92-3b03bcbae7cd resume=/dev/hda1 panic=30 splash=silent
bootsplash: silent mode.
mapped APIC to ffffb000 (fee00000)
mapped IOAPIC to ffffa000 (fec00000)
Enabling fast FPU save and restore... done.
Enabling unmasked SIMD FPU exception support... done.
Initializing CPU#0
PID hash table entries: 2048 (order: 11, 8192 bytes)
Detected 897.311 MHz processor.
Console: colour VGA+ 80x25
console [tty0] enabled
Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)
Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)
Memory: 285864k/293824k available (2268k kernel code, 7384k reserved, 778k data, 392k init, 0k highmem)
virtual kernel memory layout:
    fixmap  : 0xffe13000 - 0xfffff000   (1968 kB)
    pkmap   : 0xff800000 - 0xffc00000   (4096 kB)
    vmalloc : 0xd2800000 - 0xff7fe000   ( 719 MB)
    lowmem  : 0xc0000000 - 0xd1ef0000   ( 286 MB)
      .init : 0xc0501000 - 0xc0563000   ( 392 kB)
      .data : 0xc04370ae - 0xc04f9ba0   ( 778 kB)
      .text : 0xc0200000 - 0xc04370ae   (2268 kB)
Checking if this processor honours the WP bit even in supervisor mode...Ok.
CPA: page pool initialized 1 of 1 pages preallocated
Calibrating delay using timer specific routine.. 1796.59 BogoMIPS (lpj=3593190)
Security Framework initialized
SELinux:  Disabled at boot.
Capability LSM initialized
Mount-cache hash table entries: 512
Initializing cgroup subsys ns
Initializing cgroup subsys cpuacct
CPU: L1 I cache: 16K, L1 D cache: 16K
CPU: L2 cache: 128K
Intel machine check architecture supported.
Intel machine check reporting enabled on CPU#0.
Compat vDSO mapped to ffffe000.
Checking 'hlt' instruction... OK.
SMP alternatives: switching to UP code
Freeing SMP alternatives: 17k freed
ACPI: Core revision 20070126
CPU0: Intel Celeron (Coppermine) stepping 0a
Total of 1 processors activated (1796.59 BogoMIPS).
ENABLING IO-APIC IRQs
..TIMER: vector=0x31 apic1=0 pin1=2 apic2=-1 pin2=-1
Brought up 1 CPUs
sizeof(vma)=84 bytes
sizeof(page)=32 bytes
sizeof(inode)=340 bytes
sizeof(dentry)=132 bytes
sizeof(ext3inode)=492 bytes
sizeof(buffer_head)=56 bytes
sizeof(skbuff)=180 bytes
sizeof(task_struct)=1808 bytes
CPU0 attaching sched-domain:
 domain 0: span 00000001
  groups: 00000001
net_namespace: 548 bytes
Booting paravirtualized kernel on bare hardware
NET: Registered protocol family 16
EISA bus registered
ACPI: bus type pci registered
PCI: PCI BIOS revision 2.10 entry at 0xfb130, last bus=1
PCI: Using configuration type 1
Setting up standard PCI resources
ACPI: EC: Look up EC in DSDT
ACPI: Interpreter enabled
ACPI: (supports S0 S1 S4 S5)
ACPI: Using IOAPIC for interrupt routing
ACPI: PCI Root Bridge [PCI0] (0000:00)
pci 0000:00:1f.0: quirk: region 4000-407f claimed by ICH4 ACPI/GPIO/TCO
pci 0000:00:1f.0: quirk: region 4080-40bf claimed by ICH4 GPIO
PCI: Transparent bridge - 0000:00:1e.0
ACPI: PCI Interrupt Routing Table [\_SB_.PCI0._PRT]
ACPI: PCI Interrupt Routing Table [\_SB_.PCI0.HUB0._PRT]
ACPI: PCI Interrupt Link [LNKA] (IRQs 3 4 5 6 7 9 *10 11 12 14 15)
ACPI: PCI Interrupt Link [LNKB] (IRQs 3 4 5 6 7 9 10 11 12 14 15) *0, disabled.
ACPI: PCI Interrupt Link [LNKC] (IRQs 3 4 5 6 7 9 10 *11 12 14 15)
ACPI: PCI Interrupt Link [LNKD] (IRQs 3 4 *5 6 7 9 10 11 12 14 15)
ACPI: PCI Interrupt Link [LNKE] (IRQs 3 4 5 6 7 9 10 11 12 14 15) *0, disabled.
ACPI: PCI Interrupt Link [LNKF] (IRQs 3 4 5 6 7 9 10 11 12 14 15) *0, disabled.
ACPI: PCI Interrupt Link [LNK0] (IRQs 3 4 5 6 7 9 10 11 12 14 15) *0, disabled.
ACPI: PCI Interrupt Link [LNK1] (IRQs 3 4 5 6 7 9 10 11 *12 14 15)
Linux Plug and Play Support v0.97 (c) Adam Belay
pnp: PnP ACPI init
ACPI: bus type pnp registered
 00:00: mem resource (0xca000-0xcbfff) overlaps 0000:01:00.0 BAR 6 (0x0-0xfffff), disabling
 00:00: mem resource (0xf0000-0xf7fff) overlaps 0000:01:00.0 BAR 6 (0x0-0xfffff), disabling
 00:00: mem resource (0xf8000-0xfbfff) overlaps 0000:01:00.0 BAR 6 (0x0-0xfffff), disabling
 00:00: mem resource (0xfc000-0xfffff) overlaps 0000:01:00.0 BAR 6 (0x0-0xfffff), disabling
 00:00: mem resource (0x0-0x9ffff) overlaps 0000:01:00.0 BAR 6 (0x0-0xfffff), disabling
 00:00: mem resource (0xe0000-0xeffff) overlaps 0000:01:00.0 BAR 6 (0x0-0xfffff), disabling
pnp: PnP ACPI: found 9 devices
ACPI: ACPI bus type pnp unregistered
PnPBIOS: Disabled by ACPI PNP
PCI: Using ACPI for IRQ routing
PCI: If a device doesn't work, try "pci=routeirq".  If it helps, post a report
NetLabel: Initializing
NetLabel:  domain hash size = 128
NetLabel:  protocols = UNLABELED CIPSOv4
NetLabel:  unlabeled traffic allowed by default
ACPI: RTC can wake from S4
system 00:00: iomem range 0x11ef0000-0x11efffff could not be reserved
system 00:00: iomem range 0x100000-0x11eeffff could not be reserved
system 00:00: iomem range 0xfec00000-0xfec00fff could not be reserved
system 00:00: iomem range 0xfee00000-0xfee00fff could not be reserved
system 00:00: iomem range 0xffb00000-0xffb7ffff could not be reserved
system 00:00: iomem range 0xfff00000-0xffffffff could not be reserved
system 00:02: ioport range 0xb78-0xb7b has been reserved
system 00:02: ioport range 0xf78-0xf7b has been reserved
system 00:02: ioport range 0xa78-0xa7b has been reserved
system 00:02: ioport range 0xe78-0xe7b has been reserved
system 00:02: ioport range 0xbbc-0xbbf has been reserved
system 00:02: ioport range 0xfbc-0xfbf has been reserved
system 00:02: ioport range 0x4d0-0x4d1 has been reserved
system 00:02: ioport range 0x290-0x29f has been reserved
PCI: Bridge: 0000:00:1e.0
  IO window: c000-cfff
  MEM window: 0xe4000000-0xe5ffffff
  PREFETCH window: 0x00000000e6000000-0x00000000e60fffff
PCI: Setting latency timer of device 0000:00:1e.0 to 64
NET: Registered protocol family 2
IP route cache hash table entries: 4096 (order: 2, 16384 bytes)
TCP established hash table entries: 16384 (order: 5, 131072 bytes)
TCP bind hash table entries: 16384 (order: 5, 131072 bytes)
TCP: Hash tables configured (established 16384 bind 16384)
TCP reno registered
checking if image is initramfs... it is
Freeing initrd memory: 526k freed
audit: initializing netlink socket (disabled)
type=2000 audit(1237596596.455:1): initialized
Total HugeTLB memory allocated, 0
VFS: Disk quotas dquot_6.5.1
Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
Block layer SCSI generic (bsg) driver version 0.4 loaded (major 254)
io scheduler noop registered
io scheduler cfq registered (default)
pci 0000:00:02.0: Boot video device
pci 0000:01:00.0: Firmware left e100 interrupts enabled; disabling
isapnp: Scanning for PnP cards...
isapnp: No Plug & Play device found
Switched to high resolution mode on CPU 0
Serial: 8250/16550 driver $Revision: 1.90 $ 4 ports, IRQ sharing enabled
serial8250: ttyS0 at I/O 0x3f8 (irq = 4) is a 16550A
serial8250: ttyS1 at I/O 0x2f8 (irq = 3) is a 16550A
00:07: ttyS0 at I/O 0x3f8 (irq = 4) is a 16550A
00:08: ttyS1 at I/O 0x2f8 (irq = 3) is a 16550A
brd: module loaded
input: Macintosh mouse button emulation as /devices/virtual/input/input0
PNP: No PS/2 controller found. Probing ports directly.
serio: i8042 KBD port at 0x60,0x64 irq 1
mice: PS/2 mouse device common for all mice
EISA: Probing bus 0 at eisa.0
cpuidle: using governor ladder
cpuidle: using governor menu
TCP bic registered
NET: Registered protocol family 1
Using IPI No-Shortcut mode
registered taskstats version 1
Freeing unused kernel memory: 392k freed
Write protecting the kernel read-only data: 588k
Executing init=/init
Uniform Multi-Platform E-IDE driver
ide: Assuming 33MHz system bus speed for PIO modes; override with idebus=xx
ICH2: IDE controller (0x8086:0x244b rev 0x05) at  PCI slot 0000:00:1f.1
ICH2: not 100% native mode: will probe irqs later
    ide0: BM-DMA at 0xf000-0xf007, BIOS settings: hda:DMA, hdb:PIO
    ide1: BM-DMA at 0xf008-0xf00f, BIOS settings: hdc:PIO, hdd:PIO
Probing IDE interface ide0...
hda: ST3160215A, ATA DISK drive
hda: host max PIO4 wanted PIO255(auto-tune) selected PIO4
hda: UDMA/100 mode selected
Probing IDE interface ide1...
ide0 at 0x1f0-0x1f7,0x3f6 on irq 14
hda: max request size: 512KiB
Probing IDE interface ide1...
hda: 312581808 sectors (160041 MB) w/2048KiB Cache, CHS=19457/255/63
hda: cache flushes supported
 hda: hda1 hda2 hda4 < hda5 >
SCSI subsystem initialized
Driver 'sd' needs updating - please use bus_type methods
No dock devices found.
libata version 3.00 loaded.
PM: Starting manual resume from disk
kjournald starting.  Commit interval 5 seconds
EXT3-fs: mounted filesystem with ordered data mode.
ath_hal: module license 'Proprietary' taints kernel.
ath_hal: 0.9.18.0 (AR5210, AR5211, AR5212, RF5111, RF5112, RF2413, RF5413)
wlan: 0.9.4
ath_pci: 0.9.4
ACPI: PCI Interrupt 0000:01:02.0[A] -> GSI 18 (level, low) -> IRQ 18
ath_rate_sample: 1.2 (0.9.4)
wifi0: 11b rates: 1Mbps 2Mbps 5.5Mbps 11Mbps
wifi0: 11g rates: 1Mbps 2Mbps 5.5Mbps 11Mbps 6Mbps 9Mbps 12Mbps 18Mbps 24Mbps 36Mbps 48Mbps 54Mbps
wifi0: turboG rates: 6Mbps 12Mbps 18Mbps 24Mbps 36Mbps 48Mbps 54Mbps
wifi0: H/W encryption support: WEP AES AES_CCM TKIP
wifi0: mac 7.9 phy 4.5 radio 5.6
wifi0: Use hw queue 1 for WME_AC_BE traffic
wifi0: Use hw queue 0 for WME_AC_BK traffic
wifi0: Use hw queue 2 for WME_AC_VI traffic
wifi0: Use hw queue 3 for WME_AC_VO traffic
wifi0: Use hw queue 8 for CAB traffic
wifi0: Use hw queue 9 for beacons
wifi0: Atheros 5212: mem=0xe5100000, irq=18
ACPI: ACPI0007:00 is registered as cooling_device0
input: Power Button (FF) as /devices/LNXSYSTM:00/LNXPWRBN:00/input/input1
ACPI: Power Button (FF) [PWRF]
input: Power Button (CM) as /devices/LNXSYSTM:00/device:00/PNP0C0C:00/input/input2
ACPI: Power Button (CM) [PWRB]
input: Sleep Button (CM) as /devices/LNXSYSTM:00/device:00/PNP0C0E:00/input/input3
ACPI: Sleep Button (CM) [SLPB]
ACPI: LNXTHERM:01 is registered as thermal_zone0
ACPI: Thermal Zone [THRM] (42 C)
ACPI: PNP0C0B:00 is registered as cooling_device1
ACPI: Fan [FAN] (on)
Linux agpgart interface v0.103
agpgart: Detected an Intel i815 Chipset.
agpgart: AGP aperture is 64M @ 0xe0000000
i810_smbus 0000:00:02.0: i810/i815 i2c device found.
ACPI: PCI Interrupt 0000:00:1f.3[B] -> GSI 17 (level, low) -> IRQ 17
usbcore: registered new interface driver usbfs
usbcore: registered new interface driver hub
usbcore: registered new device driver usb
input: PC Speaker as /devices/platform/pcspkr/input/input4
e100: Intel(R) PRO/100 Network Driver, 3.5.23-k4-NAPI
e100: Copyright(c) 1999-2006 Intel Corporation
ACPI: PCI Interrupt 0000:01:00.0[A] -> GSI 16 (level, low) -> IRQ 16
e100: eth0: e100_probe: addr 0xe6000000, irq 16, MAC addr 00:a0:c9:4b:b8:41
USB Universal Host Controller Interface driver v3.0
ACPI: PCI Interrupt 0000:00:1f.2[D] -> GSI 19 (level, low) -> IRQ 19
PCI: Setting latency timer of device 0000:00:1f.2 to 64
uhci_hcd 0000:00:1f.2: UHCI Host Controller
uhci_hcd 0000:00:1f.2: new USB bus registered, assigned bus number 1
uhci_hcd 0000:00:1f.2: irq 19, io base 0x0000d000
usb usb1: configuration #1 chosen from 1 choice
hub 1-0:1.0: USB hub found
hub 1-0:1.0: 2 ports detected
usb usb1: New USB device found, idVendor=1d6b, idProduct=0001
usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
usb usb1: Product: UHCI Host Controller
usb usb1: Manufacturer: Linux 2.6.25-std-def-alt8.M41.4 uhci_hcd
usb usb1: SerialNumber: 0000:00:1f.2
ACPI: PCI Interrupt 0000:00:1f.4[C] -> GSI 23 (level, low) -> IRQ 23
PCI: Setting latency timer of device 0000:00:1f.4 to 64
uhci_hcd 0000:00:1f.4: UHCI Host Controller
uhci_hcd 0000:00:1f.4: new USB bus registered, assigned bus number 2
uhci_hcd 0000:00:1f.4: irq 23, io base 0x0000d400
usb usb2: configuration #1 chosen from 1 choice
hub 2-0:1.0: USB hub found
hub 2-0:1.0: 2 ports detected
usb usb2: New USB device found, idVendor=1d6b, idProduct=0001
usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
usb usb2: Product: UHCI Host Controller
usb usb2: Manufacturer: Linux 2.6.25-std-def-alt8.M41.4 uhci_hcd
usb usb2: SerialNumber: 0000:00:1f.4
Real Time Clock Driver v1.12ac
Adding 570268k swap on /dev/hda1.  Priority:-1 extents:1 across:570268k
EXT3 FS on hda2, internal journal
hda: UDMA/100 mode selected
device-mapper: uevent: version 1.0.3
device-mapper: ioctl: 4.13.0-ioctl (2007-10-18) initialised: dm-devel@redhat.com
kjournald starting.  Commit interval 5 seconds
EXT3 FS on hda5, internal journal
EXT3-fs: mounted filesystem with ordered data mode.
