X Window System Version 7.2.0
Release Date: 05 February 2007
X Protocol Version 11, Revision 0, Release 7.2
Build Operating System: Linux 2.6.18-std-smp-alt3 x86_64 ALT Linux
Current Operating System: Linux localhost.localdomain 2.6.18-std-smp-alt4 #1 SMP Fri Feb 16 19:41:21 MSK 2007 x86_64
Build Date: 05 February 2007
	Before reporting problems, check https://bugzilla.altlinux.org/
	to make sure that you have the latest version.
Module Loader present
Markers: (--) probed, (**) from config file, (==) default setting,
	(++) from command line, (!!) notice, (II) informational,
	(WW) warning, (EE) error, (NI) not implemented, (??) unknown.
(++) Log file: "/tmp/x11.log", Time: Fri Feb 23 12:37:40 2007
(==) Using config file: "/etc/X11/xorg.conf"
(==) ServerLayout "Minimal layout"
(**) |-->Screen "Screen0" (0)
(**) |   |-->Monitor "Monitor0"
(**) |   |-->Device "Card0|0"
(**) |-->Input Device "Mouse0"
(**) |-->Input Device "Keyboard0"
(==) FontPath set to:
	/usr/share/fonts/bitmap/misc/
(==) RgbPath set to "/usr/share/X11/rgb"
(==) ModulePath set to "/usr/lib64/X11/modules"
(II) Loader magic: 0x7a7c40
(II) Module ABI versions:
	X.Org ANSI C Emulation: 0.3
	X.Org Video Driver: 1.1
	X.Org XInput driver : 0.7
	X.Org Server Extension : 0.3
	X.Org Font Renderer : 0.5
(II) Loader running on linux
(II) LoadModule: "pcidata"
(II) Loading /usr/lib64/X11/modules//libpcidata.so
(II) Module pcidata: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	ABI class: X.Org Video Driver, version 1.1
(++) using VT number 7

(II) PCI: PCI scan (all values are in hex)
(II) PCI: 00:00:0: chip 10de,02f0 card 1043,81c0 rev a2 class 05,00,00 hdr 80
(II) PCI: 00:00:1: chip 10de,02fa card 1043,81c0 rev a2 class 05,00,00 hdr 80
(II) PCI: 00:00:2: chip 10de,02fe card 1043,81c0 rev a2 class 05,00,00 hdr 80
(II) PCI: 00:00:3: chip 10de,02f8 card 1043,81c0 rev a2 class 05,00,00 hdr 80
(II) PCI: 00:00:4: chip 10de,02f9 card 1043,81c0 rev a2 class 05,00,00 hdr 00
(II) PCI: 00:00:5: chip 10de,02ff card 1043,81c0 rev a2 class 05,00,00 hdr 80
(II) PCI: 00:00:6: chip 10de,027f card 1043,81c0 rev a2 class 05,00,00 hdr 80
(II) PCI: 00:00:7: chip 10de,027e card 1043,81c0 rev a2 class 05,00,00 hdr 80
(II) PCI: 00:02:0: chip 10de,02fc card 0000,0000 rev a1 class 06,04,00 hdr 01
(II) PCI: 00:03:0: chip 10de,02fd card 0000,0000 rev a1 class 06,04,00 hdr 01
(II) PCI: 00:04:0: chip 10de,02fb card 0000,0000 rev a1 class 06,04,00 hdr 01
(II) PCI: 00:05:0: chip 10de,0240 card 1043,81cd rev a2 class 03,00,00 hdr 00
(II) PCI: 00:09:0: chip 10de,0270 card 1043,81c0 rev a2 class 05,00,00 hdr 00
(II) PCI: 00:0a:0: chip 10de,0260 card 1043,81c0 rev a3 class 06,01,00 hdr 80
(II) PCI: 00:0a:1: chip 10de,0264 card 1043,81c0 rev a3 class 0c,05,00 hdr 80
(II) PCI: 00:0a:2: chip 10de,0272 card 1043,81c0 rev a3 class 05,00,00 hdr 80
(II) PCI: 00:0b:0: chip 10de,026d card 1043,81c0 rev a3 class 0c,03,10 hdr 80
(II) PCI: 00:0b:1: chip 10de,026e card 1043,81c0 rev a3 class 0c,03,20 hdr 80
(II) PCI: 00:0d:0: chip 10de,0265 card 1043,81c0 rev a1 class 01,01,8a hdr 00
(II) PCI: 00:0e:0: chip 10de,0266 card 1043,81c0 rev a1 class 01,01,85 hdr 00
(II) PCI: 00:10:0: chip 10de,026f card 0000,0000 rev a2 class 06,04,01 hdr 81
(II) PCI: 00:10:1: chip 10de,026c card 1043,81cb rev a2 class 04,03,00 hdr 80
(II) PCI: 00:14:0: chip 10de,0269 card 1043,816a rev a3 class 06,80,00 hdr 00
(II) PCI: 00:18:0: chip 1022,1100 card 0000,0000 rev 00 class 06,00,00 hdr 80
(II) PCI: 00:18:1: chip 1022,1101 card 0000,0000 rev 00 class 06,00,00 hdr 80
(II) PCI: 00:18:2: chip 1022,1102 card 0000,0000 rev 00 class 06,00,00 hdr 80
(II) PCI: 00:18:3: chip 1022,1103 card 0000,0000 rev 00 class 06,00,00 hdr 80
(II) PCI: 04:05:0: chip 104c,8023 card 1043,808b rev 00 class 0c,00,10 hdr 00
(II) PCI: 04:08:0: chip 1319,0801 card 1319,1319 rev b2 class 04,01,00 hdr 80
(II) PCI: 04:08:1: chip 1319,0802 card 1319,1319 rev b2 class 09,80,00 hdr 80
(II) PCI: End of PCI scan
(II) PCI-to-PCI bridge:
(II) Bus 1: bridge is at (0:2:0), (0,1,1), BCTRL: 0x0004 (VGA_EN is cleared)
(II) Bus 1 I/O range:
	[0] -1	0	0x0000c000 - 0x0000c0ff (0x100) IX[B]
	[1] -1	0	0x0000c400 - 0x0000c4ff (0x100) IX[B]
	[2] -1	0	0x0000c800 - 0x0000c8ff (0x100) IX[B]
	[3] -1	0	0x0000cc00 - 0x0000ccff (0x100) IX[B]
(II) Bus 1 non-prefetchable memory range:
	[0] -1	0	0xfd700000 - 0xfd7fffff (0x100000) MX[B]
(II) Bus 1 prefetchable memory range:
	[0] -1	0	0xfde00000 - 0xfdefffff (0x100000) MX[B]
(II) PCI-to-PCI bridge:
(II) Bus 2: bridge is at (0:3:0), (0,2,2), BCTRL: 0x0004 (VGA_EN is cleared)
(II) Bus 2 I/O range:
	[0] -1	0	0x0000b000 - 0x0000b0ff (0x100) IX[B]
	[1] -1	0	0x0000b400 - 0x0000b4ff (0x100) IX[B]
	[2] -1	0	0x0000b800 - 0x0000b8ff (0x100) IX[B]
	[3] -1	0	0x0000bc00 - 0x0000bcff (0x100) IX[B]
(II) Bus 2 non-prefetchable memory range:
	[0] -1	0	0xfdd00000 - 0xfddfffff (0x100000) MX[B]
(II) Bus 2 prefetchable memory range:
	[0] -1	0	0xfdc00000 - 0xfdcfffff (0x100000) MX[B]
(II) PCI-to-PCI bridge:
(II) Bus 3: bridge is at (0:4:0), (0,3,3), BCTRL: 0x0004 (VGA_EN is cleared)
(II) Bus 3 I/O range:
	[0] -1	0	0x00009000 - 0x000090ff (0x100) IX[B]
	[1] -1	0	0x00009400 - 0x000094ff (0x100) IX[B]
	[2] -1	0	0x00009800 - 0x000098ff (0x100) IX[B]
	[3] -1	0	0x00009c00 - 0x00009cff (0x100) IX[B]
(II) Bus 3 non-prefetchable memory range:
	[0] -1	0	0xfd900000 - 0xfd9fffff (0x100000) MX[B]
(II) Bus 3 prefetchable memory range:
	[0] -1	0	0xfd800000 - 0xfd8fffff (0x100000) MX[B]
(II) PCI-to-ISA bridge:
(II) Bus -1: bridge is at (0:10:0), (0,-1,-1), BCTRL: 0x0008 (VGA_EN is set)
(II) Subtractive PCI-to-PCI bridge:
(II) Bus 4: bridge is at (0:16:0), (0,4,4), BCTRL: 0x0204 (VGA_EN is cleared)
(II) Bus 4 I/O range:
	[0] -1	0	0x0000a000 - 0x0000a0ff (0x100) IX[B]
	[1] -1	0	0x0000a400 - 0x0000a4ff (0x100) IX[B]
	[2] -1	0	0x0000a800 - 0x0000a8ff (0x100) IX[B]
	[3] -1	0	0x0000ac00 - 0x0000acff (0x100) IX[B]
(II) Bus 4 non-prefetchable memory range:
	[0] -1	0	0xfdb00000 - 0xfdbfffff (0x100000) MX[B]
(II) Bus 4 prefetchable memory range:
	[0] -1	0	0xfda00000 - 0xfdafffff (0x100000) MX[B]
(II) Host-to-PCI bridge:
(II) Bus 0: bridge is at (0:24:0), (0,0,4), BCTRL: 0x0008 (VGA_EN is set)
(II) Bus 0 I/O range:
	[0] -1	0	0x00000000 - 0x0000ffff (0x10000) IX[B]
(II) Bus 0 non-prefetchable memory range:
	[0] -1	0	0x00000000 - 0xffffffff (0x100000000) MX[B]
(II) Bus 0 prefetchable memory range:
	[0] -1	0	0x00000000 - 0xffffffff (0x100000000) MX[B]
(--) PCI:*(0:5:0) nVidia Corporation C51PV [GeForce 6150] rev 162, Mem @ 0xfb000000/24, 0xd0000000/28, 0xfc000000/24
(II) Addressable bus resource ranges are
	[0] -1	0	0x00000000 - 0xffffffff (0x100000000) MX[B]
	[1] -1	0	0x00000000 - 0x0000ffff (0x10000) IX[B]
(II) OS-reported resource ranges:
	[0] -1	0	0x00100000 - 0x3fffffff (0x3ff00000) MX[B]E(B)
	[1] -1	0	0x000f0000 - 0x000fffff (0x10000) MX[B]
	[2] -1	0	0x000c0000 - 0x000effff (0x30000) MX[B]
	[3] -1	0	0x00000000 - 0x0009ffff (0xa0000) MX[B]
	[4] -1	0	0x0000ffff - 0x0000ffff (0x1) IX[B]
	[5] -1	0	0x00000000 - 0x000000ff (0x100) IX[B]
(II) Active PCI resource ranges:
	[0] -1	0	0xfdbf8000 - 0xfdbfbfff (0x4000) MX[B]
	[1] -1	0	0xfdbff000 - 0xfdbff7ff (0x800) MX[B]
	[2] -1	0	0xfe02c000 - 0xfe02cfff (0x1000) MX[B]
	[3] -1	0	0xfe028000 - 0xfe02bfff (0x4000) MX[B]
	[4] -1	0	0xfe02d000 - 0xfe02dfff (0x1000) MX[B]
	[5] -1	0	0xfe02e000 - 0xfe02e0ff (0x100) MX[B]
	[6] -1	0	0xfe02f000 - 0xfe02ffff (0x1000) MX[B]
	[7] -1	0	0xfc000000 - 0xfcffffff (0x1000000) MX[B](B)
	[8] -1	0	0xd0000000 - 0xdfffffff (0x10000000) MX[B](B)
	[9] -1	0	0xfb000000 - 0xfbffffff (0x1000000) MX[B](B)
	[10] -1	0	0x0000a800 - 0x0000a80f (0x10) IX[B]
	[11] -1	0	0x0000ac00 - 0x0000ac7f (0x80) IX[B]
	[12] -1	0	0x0000dc00 - 0x0000dc07 (0x8) IX[B]
	[13] -1	0	0x0000e000 - 0x0000e00f (0x10) IX[B]
	[14] -1	0	0x00000b70 - 0x00000b73 (0x4) IX[B]
	[15] -1	0	0x00000970 - 0x00000977 (0x8) IX[B]
	[16] -1	0	0x00000bf0 - 0x00000bf3 (0x4) IX[B]
	[17] -1	0	0x000009f0 - 0x000009f7 (0x8) IX[B]
	[18] -1	0	0x0000f400 - 0x0000f40f (0x10) IX[B]
	[19] -1	0	0x00004c40 - 0x00004c7f (0x40) IX[B]
	[20] -1	0	0x00004c00 - 0x00004c3f (0x40) IX[B]
(II) Active PCI resource ranges after removing overlaps:
	[0] -1	0	0xfdbf8000 - 0xfdbfbfff (0x4000) MX[B]
	[1] -1	0	0xfdbff000 - 0xfdbff7ff (0x800) MX[B]
	[2] -1	0	0xfe02c000 - 0xfe02cfff (0x1000) MX[B]
	[3] -1	0	0xfe028000 - 0xfe02bfff (0x4000) MX[B]
	[4] -1	0	0xfe02d000 - 0xfe02dfff (0x1000) MX[B]
	[5] -1	0	0xfe02e000 - 0xfe02e0ff (0x100) MX[B]
	[6] -1	0	0xfe02f000 - 0xfe02ffff (0x1000) MX[B]
	[7] -1	0	0xfc000000 - 0xfcffffff (0x1000000) MX[B](B)
	[8] -1	0	0xd0000000 - 0xdfffffff (0x10000000) MX[B](B)
	[9] -1	0	0xfb000000 - 0xfbffffff (0x1000000) MX[B](B)
	[10] -1	0	0x0000a800 - 0x0000a80f (0x10) IX[B]
	[11] -1	0	0x0000ac00 - 0x0000ac7f (0x80) IX[B]
	[12] -1	0	0x0000dc00 - 0x0000dc07 (0x8) IX[B]
	[13] -1	0	0x0000e000 - 0x0000e00f (0x10) IX[B]
	[14] -1	0	0x00000b70 - 0x00000b73 (0x4) IX[B]
	[15] -1	0	0x00000970 - 0x00000977 (0x8) IX[B]
	[16] -1	0	0x00000bf0 - 0x00000bf3 (0x4) IX[B]
	[17] -1	0	0x000009f0 - 0x000009f7 (0x8) IX[B]
	[18] -1	0	0x0000f400 - 0x0000f40f (0x10) IX[B]
	[19] -1	0	0x00004c40 - 0x00004c7f (0x40) IX[B]
	[20] -1	0	0x00004c00 - 0x00004c3f (0x40) IX[B]
(II) OS-reported resource ranges after removing overlaps with PCI:
	[0] -1	0	0x00100000 - 0x3fffffff (0x3ff00000) MX[B]E(B)
	[1] -1	0	0x000f0000 - 0x000fffff (0x10000) MX[B]
	[2] -1	0	0x000c0000 - 0x000effff (0x30000) MX[B]
	[3] -1	0	0x00000000 - 0x0009ffff (0xa0000) MX[B]
	[4] -1	0	0x0000ffff - 0x0000ffff (0x1) IX[B]
	[5] -1	0	0x00000000 - 0x000000ff (0x100) IX[B]
(II) All system resource ranges:
	[0] -1	0	0x00100000 - 0x3fffffff (0x3ff00000) MX[B]E(B)
	[1] -1	0	0x000f0000 - 0x000fffff (0x10000) MX[B]
	[2] -1	0	0x000c0000 - 0x000effff (0x30000) MX[B]
	[3] -1	0	0x00000000 - 0x0009ffff (0xa0000) MX[B]
	[4] -1	0	0xfdbf8000 - 0xfdbfbfff (0x4000) MX[B]
	[5] -1	0	0xfdbff000 - 0xfdbff7ff (0x800) MX[B]
	[6] -1	0	0xfe02c000 - 0xfe02cfff (0x1000) MX[B]
	[7] -1	0	0xfe028000 - 0xfe02bfff (0x4000) MX[B]
	[8] -1	0	0xfe02d000 - 0xfe02dfff (0x1000) MX[B]
	[9] -1	0	0xfe02e000 - 0xfe02e0ff (0x100) MX[B]
	[10] -1	0	0xfe02f000 - 0xfe02ffff (0x1000) MX[B]
	[11] -1	0	0xfc000000 - 0xfcffffff (0x1000000) MX[B](B)
	[12] -1	0	0xd0000000 - 0xdfffffff (0x10000000) MX[B](B)
	[13] -1	0	0xfb000000 - 0xfbffffff (0x1000000) MX[B](B)
	[14] -1	0	0x0000ffff - 0x0000ffff (0x1) IX[B]
	[15] -1	0	0x00000000 - 0x000000ff (0x100) IX[B]
	[16] -1	0	0x0000a800 - 0x0000a80f (0x10) IX[B]
	[17] -1	0	0x0000ac00 - 0x0000ac7f (0x80) IX[B]
	[18] -1	0	0x0000dc00 - 0x0000dc07 (0x8) IX[B]
	[19] -1	0	0x0000e000 - 0x0000e00f (0x10) IX[B]
	[20] -1	0	0x00000b70 - 0x00000b73 (0x4) IX[B]
	[21] -1	0	0x00000970 - 0x00000977 (0x8) IX[B]
	[22] -1	0	0x00000bf0 - 0x00000bf3 (0x4) IX[B]
	[23] -1	0	0x000009f0 - 0x000009f7 (0x8) IX[B]
	[24] -1	0	0x0000f400 - 0x0000f40f (0x10) IX[B]
	[25] -1	0	0x00004c40 - 0x00004c7f (0x40) IX[B]
	[26] -1	0	0x00004c00 - 0x00004c3f (0x40) IX[B]
(II) LoadModule: "type1"
(II) Loading /usr/lib64/X11/modules/fonts//libtype1.so
(II) Module type1: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.2
	Module class: X.Org Font Renderer
	ABI class: X.Org Font Renderer, version 0.5
(II) Loading font Type1
(II) LoadModule: "freetype"
(II) Loading /usr/lib64/X11/modules/fonts//libfreetype.so
(II) Module freetype: vendor="X.Org Foundation & the After X-TT Project"
	compiled for 7.2.0, module version = 2.1.0
	Module class: X.Org Font Renderer
	ABI class: X.Org Font Renderer, version 0.5
(II) Loading font FreeType
(II) LoadModule: "glx"
(II) Loading /usr/lib64/X11/modules/extensions//libglx.so
(II) Module glx: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	ABI class: X.Org Server Extension, version 0.3
(==) AIGLX disabled
(II) Loading extension GLX
(II) LoadModule: "dri"
(II) Loading /usr/lib64/X11/modules/extensions//libdri.so
(II) Module dri: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	ABI class: X.Org Server Extension, version 0.3
(II) Loading extension XFree86-DRI
(II) LoadModule: "dbe"
(II) Loading /usr/lib64/X11/modules/extensions//libdbe.so
(II) Module dbe: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	Module class: X.Org Server Extension
	ABI class: X.Org Server Extension, version 0.3
(II) Loading extension DOUBLE-BUFFER
(II) LoadModule: "extmod"
(II) Loading /usr/lib64/X11/modules/extensions//libextmod.so
(II) Module extmod: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	Module class: X.Org Server Extension
	ABI class: X.Org Server Extension, version 0.3
(II) Loading extension SHAPE
(II) Loading extension MIT-SUNDRY-NONSTANDARD
(II) Loading extension BIG-REQUESTS
(II) Loading extension SYNC
(II) Loading extension MIT-SCREEN-SAVER
(II) Loading extension XC-MISC
(II) Loading extension XFree86-VidModeExtension
(II) Loading extension XFree86-Misc
(II) Loading extension DPMS
(II) Loading extension TOG-CUP
(II) Loading extension Extended-Visual-Information
(II) Loading extension XVideo
(II) Loading extension XVideo-MotionCompensation
(II) Loading extension X-Resource
(II) LoadModule: "nv"
(II) Loading /usr/lib64/X11/modules/drivers//nv_drv.so
(II) Module nv: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.2.2
	Module class: X.Org Video Driver
	ABI class: X.Org Video Driver, version 1.1
(II) LoadModule: "mouse"
(II) Loading /usr/lib64/X11/modules/input//mouse_drv.so
(II) Module mouse: vendor="X.Org Foundation"
	compiled for 7.1.99.902, module version = 1.1.1
	Module class: X.Org XInput Driver
	ABI class: X.Org XInput driver, version 0.6
(II) LoadModule: "kbd"
(II) Loading /usr/lib64/X11/modules/input//kbd_drv.so
(II) Module kbd: vendor="X.Org Foundation"
	compiled for 7.1.99.903, module version = 1.1.0
	Module class: X.Org XInput Driver
	ABI class: X.Org XInput driver, version 0.6
(II) NV: driver for NVIDIA chipsets: RIVA 128, RIVA TNT, RIVA TNT2,
	Unknown TNT2, Vanta, RIVA TNT2 Ultra, RIVA TNT2 Model 64,
	Aladdin TNT2, GeForce 256, GeForce DDR, Quadro, GeForce2 MX/MX 400,
	GeForce2 MX 100/200, GeForce2 Go, Quadro2 MXR/EX/Go,
	GeForce2 Integrated GPU, GeForce2 GTS, GeForce2 Ti, GeForce2 Ultra,
	Quadro2 Pro, GeForce4 MX 460, GeForce4 MX 440, GeForce4 MX 420,
	GeForce4 MX 440-SE, GeForce4 440 Go, GeForce4 420 Go,
	GeForce4 420 Go 32M, GeForce4 460 Go, Quadro4 550 XGL,
	GeForce4 440 Go 64M, Quadro NVS, Quadro4 500 GoGL,
	GeForce4 410 Go 16M, GeForce4 MX 440 with AGP8X,
	GeForce4 MX 440SE with AGP8X, GeForce4 MX 420 with AGP8X,
	GeForce4 MX 4000, GeForce4 448 Go, GeForce4 488 Go, Quadro4 580 XGL,
	Quadro4 NVS 280 SD, Quadro4 380 XGL, Quadro NVS 50 PCI,
	GeForce4 448 Go, GeForce4 MX Integrated GPU, GeForce3,
	GeForce3 Ti 200, GeForce3 Ti 500, Quadro DCC, GeForce4 Ti 4600,
	GeForce4 Ti 4400, GeForce4 Ti 4200, Quadro4 900 XGL, Quadro4 750 XGL,
	Quadro4 700 XGL, GeForce4 Ti 4800, GeForce4 Ti 4200 with AGP8X,
	GeForce4 Ti 4800 SE, GeForce4 4200 Go, Quadro4 700 GoGL,
	Quadro4 980 XGL, Quadro4 780 XGL, GeForce FX 5800 Ultra,
	GeForce FX 5800, Quadro FX 2000, Quadro FX 1000,
	GeForce FX 5600 Ultra, GeForce FX 5600, GeForce FX 5600XT,
	GeForce FX Go5600, GeForce FX Go5650, Quadro FX Go700,
	GeForce FX 5200, GeForce FX 5200 Ultra, GeForce FX 5200,
	GeForce FX 5200LE, GeForce FX Go5200, GeForce FX Go5250,
	GeForce FX 5500, GeForce FX 5100, GeForce FX Go5200 32M/64M,
	Quadro NVS 55/280 PCI, Quadro FX 500/600 PCI,
	GeForce FX Go53xx Series, GeForce FX Go5100, GeForce FX 5900 Ultra,
	GeForce FX 5900, GeForce FX 5900XT, GeForce FX 5950 Ultra,
	GeForce FX 5900ZT, Quadro FX 3000, Quadro FX 700,
	GeForce FX 5700 Ultra, GeForce FX 5700, GeForce FX 5700LE,
	GeForce FX 5700VE, GeForce FX Go5700, GeForce FX Go5700,
	Quadro FX Go1000, Quadro FX 1100, GeForce 6800 Ultra, GeForce 6800,
	GeForce 6800 LE, GeForce 6800 XE, GeForce 6800 XT, GeForce 6800 GT,
	GeForce 6800 GT, GeForce 6800 GS, GeForce 6800 XT, Quadro FX 4000,
	GeForce 6800 GS, GeForce 6800, GeForce 6800 LE, GeForce 6800 XT,
	GeForce Go 6800, GeForce Go 6800 Ultra, Quadro FX Go1400,
	Quadro FX 3450/4000 SDI, Quadro FX 1400, GeForce 6600 GT,
	GeForce 6600, GeForce 6600 LE, GeForce 6600 VE, GeForce Go 6600,
	GeForce 6610 XL, GeForce Go 6600 TE/6200 TE, GeForce 6700 XL,
	GeForce Go 6600, GeForce Go 6600 GT, Quadro FX 550, Quadro FX 550,
	Quadro FX 540, GeForce 6200, GeForce 6500,
	GeForce 6200 TurboCache(TM), GeForce 6200SE TurboCache(TM),
	GeForce 6200 LE, GeForce Go 6200, Quadro NVS 285, GeForce Go 6400,
	GeForce Go 6200, GeForce Go 6400, GeForce 6250, GeForce 6800,
	GeForce 6800 LE, GeForce 6800 GT, GeForce 6800 XT, GeForce 6200,
	GeForce 6200 A-LE, GeForce 7800 GTX, GeForce 7800 GTX,
	GeForce 7800 GT, GeForce 7800 GS, GeForce 7800 SLI, GeForce Go 7800,
	GeForce Go 7800 GTX, Quadro FX 4500, GeForce 7300 LE,
	GeForce 7300 SE, GeForce Go 7200, GeForce Go 7300, GeForce Go 7400,
	GeForce Go 7400 GS, Quadro NVS 110M, Quadro NVS 120M, Quadro FX 350M,
	GeForce 7500 LE, Quadro FX 350, GeForce 7300 GS, GeForce 7600 GT,
	GeForce 7600 GS, GeForce 7300 GT, GeForce 7600 LE, GeForce 7300 GT,
	GeForce Go 7700, GeForce Go 7600, GeForce Go 7600 GT,
	Quadro NVS 300M, GeForce Go 7900 SE, Quadro FX 550M, Quadro FX 560,
	GeForce 7900 GTX, GeForce 7900 GT, GeForce 7900 GS,
	GeForce Go 7900 GS, GeForce Go 7900 GTX, Quadro FX 2500M,
	Quadro FX 1500M, Quadro FX 5500, Quadro FX 3500, Quadro FX 1500,
	Quadro FX 4500 X2, GeForce 6150, GeForce 6150 LE, GeForce 6100,
	GeForce Go 6150, GeForce Go 6100
(II) Primary Device is: PCI 00:05:0
(--) Assigning device section with no busID to primary device
(--) Chipset GeForce 6150 found
(II) resource ranges after xf86ClaimFixedResources() call:
	[0] -1	0	0x00100000 - 0x3fffffff (0x3ff00000) MX[B]E(B)
	[1] -1	0	0x000f0000 - 0x000fffff (0x10000) MX[B]
	[2] -1	0	0x000c0000 - 0x000effff (0x30000) MX[B]
	[3] -1	0	0x00000000 - 0x0009ffff (0xa0000) MX[B]
	[4] -1	0	0xfdbf8000 - 0xfdbfbfff (0x4000) MX[B]
	[5] -1	0	0xfdbff000 - 0xfdbff7ff (0x800) MX[B]
	[6] -1	0	0xfe02c000 - 0xfe02cfff (0x1000) MX[B]
	[7] -1	0	0xfe028000 - 0xfe02bfff (0x4000) MX[B]
	[8] -1	0	0xfe02d000 - 0xfe02dfff (0x1000) MX[B]
	[9] -1	0	0xfe02e000 - 0xfe02e0ff (0x100) MX[B]
	[10] -1	0	0xfe02f000 - 0xfe02ffff (0x1000) MX[B]
	[11] -1	0	0xfc000000 - 0xfcffffff (0x1000000) MX[B](B)
	[12] -1	0	0xd0000000 - 0xdfffffff (0x10000000) MX[B](B)
	[13] -1	0	0xfb000000 - 0xfbffffff (0x1000000) MX[B](B)
	[14] -1	0	0x0000ffff - 0x0000ffff (0x1) IX[B]
	[15] -1	0	0x00000000 - 0x000000ff (0x100) IX[B]
	[16] -1	0	0x0000a800 - 0x0000a80f (0x10) IX[B]
	[17] -1	0	0x0000ac00 - 0x0000ac7f (0x80) IX[B]
	[18] -1	0	0x0000dc00 - 0x0000dc07 (0x8) IX[B]
	[19] -1	0	0x0000e000 - 0x0000e00f (0x10) IX[B]
	[20] -1	0	0x00000b70 - 0x00000b73 (0x4) IX[B]
	[21] -1	0	0x00000970 - 0x00000977 (0x8) IX[B]
	[22] -1	0	0x00000bf0 - 0x00000bf3 (0x4) IX[B]
	[23] -1	0	0x000009f0 - 0x000009f7 (0x8) IX[B]
	[24] -1	0	0x0000f400 - 0x0000f40f (0x10) IX[B]
	[25] -1	0	0x00004c40 - 0x00004c7f (0x40) IX[B]
	[26] -1	0	0x00004c00 - 0x00004c3f (0x40) IX[B]
(II) resource ranges after probing:
	[0] -1	0	0x00100000 - 0x3fffffff (0x3ff00000) MX[B]E(B)
	[1] -1	0	0x000f0000 - 0x000fffff (0x10000) MX[B]
	[2] -1	0	0x000c0000 - 0x000effff (0x30000) MX[B]
	[3] -1	0	0x00000000 - 0x0009ffff (0xa0000) MX[B]
	[4] -1	0	0xfdbf8000 - 0xfdbfbfff (0x4000) MX[B]
	[5] -1	0	0xfdbff000 - 0xfdbff7ff (0x800) MX[B]
	[6] -1	0	0xfe02c000 - 0xfe02cfff (0x1000) MX[B]
	[7] -1	0	0xfe028000 - 0xfe02bfff (0x4000) MX[B]
	[8] -1	0	0xfe02d000 - 0xfe02dfff (0x1000) MX[B]
	[9] -1	0	0xfe02e000 - 0xfe02e0ff (0x100) MX[B]
	[10] -1	0	0xfe02f000 - 0xfe02ffff (0x1000) MX[B]
	[11] -1	0	0xfc000000 - 0xfcffffff (0x1000000) MX[B](B)
	[12] -1	0	0xd0000000 - 0xdfffffff (0x10000000) MX[B](B)
	[13] -1	0	0xfb000000 - 0xfbffffff (0x1000000) MX[B](B)
	[14] 0	0	0x000a0000 - 0x000affff (0x10000) MS[B]
	[15] 0	0	0x000b0000 - 0x000b7fff (0x8000) MS[B]
	[16] 0	0	0x000b8000 - 0x000bffff (0x8000) MS[B]
	[17] -1	0	0x0000ffff - 0x0000ffff (0x1) IX[B]
	[18] -1	0	0x00000000 - 0x000000ff (0x100) IX[B]
	[19] -1	0	0x0000a800 - 0x0000a80f (0x10) IX[B]
	[20] -1	0	0x0000ac00 - 0x0000ac7f (0x80) IX[B]
	[21] -1	0	0x0000dc00 - 0x0000dc07 (0x8) IX[B]
	[22] -1	0	0x0000e000 - 0x0000e00f (0x10) IX[B]
	[23] -1	0	0x00000b70 - 0x00000b73 (0x4) IX[B]
	[24] -1	0	0x00000970 - 0x00000977 (0x8) IX[B]
	[25] -1	0	0x00000bf0 - 0x00000bf3 (0x4) IX[B]
	[26] -1	0	0x000009f0 - 0x000009f7 (0x8) IX[B]
	[27] -1	0	0x0000f400 - 0x0000f40f (0x10) IX[B]
	[28] -1	0	0x00004c40 - 0x00004c7f (0x40) IX[B]
	[29] -1	0	0x00004c00 - 0x00004c3f (0x40) IX[B]
	[30] 0	0	0x000003b0 - 0x000003bb (0xc) IS[B]
	[31] 0	0	0x000003c0 - 0x000003df (0x20) IS[B]
(II) Setting vga for screen 0.
(II) Loading sub module "int10"
(II) LoadModule: "int10"
(II) Loading /usr/lib64/X11/modules//libint10.so
(II) Module int10: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	ABI class: X.Org Video Driver, version 1.1
(II) NV(0): Initializing int10
(II) NV(0): Primary V_BIOS segment is: 0xc000
(--) NV(0): Chipset: "GeForce 6150"
(==) NV(0): Depth 24, (==) framebuffer bpp 32
(==) NV(0): RGB weight 888
(==) NV(0): Default visual is TrueColor
(II) Loading sub module "vgahw"
(II) LoadModule: "vgahw"
(II) Loading /usr/lib64/X11/modules//libvgahw.so
(II) Module vgahw: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 0.1.0
	ABI class: X.Org Video Driver, version 1.1
(==) NV(0): Using HW cursor
(--) NV(0): Linear framebuffer at 0xD0000000
(--) NV(0): MMIO registers at 0xFB000000
(II) Loading sub module "i2c"
(II) LoadModule: "i2c"
(II) Loading /usr/lib64/X11/modules//libi2c.so
(II) Module i2c: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.2.0
	ABI class: X.Org Video Driver, version 1.1
(II) Loading sub module "ddc"
(II) LoadModule: "ddc"
(II) Loading /usr/lib64/X11/modules//libddc.so
(II) Module ddc: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	ABI class: X.Org Video Driver, version 1.1
(II) NV(0): I2C bus "DDC" initialized.
(II) NV(0): Probing for analog device on output A...
(--) NV(0):   ...can't find one
(II) NV(0): Probing for analog device on output B...
(--) NV(0):   ...can't find one
(II) NV(0): Probing for EDID on I2C bus A...
(II) NV(0): I2C device "DDC:ddc2" registered at address 0xA0.
(II) NV(0): I2C device "DDC:ddc2" removed.
(II) NV(0):   ... none found
(II) NV(0): Probing for EDID on I2C bus B...
(II) NV(0): I2C device "DDC:ddc2" registered at address 0xA0.
(II) NV(0): I2C device "DDC:ddc2" removed.
(II) NV(0):   ... none found
(--) NV(0): CRTC 0 is currently programmed for DFP
(II) NV(0): Using DFP on CRTC 0
(--) NV(0): Panel size is 1024 x 768
(II) NV(0): Panel is TMDS
(--) NV(0): VideoRAM: 32768 kBytes
(==) NV(0): Using gamma correction (1.0, 1.0, 1.0)
(II) NV(0): Monitor0: Using default hsync range of 31.50-37.90 kHz
(II) NV(0): Monitor0: Using default vrefresh range of 50.00-70.00 Hz
(II) NV(0): Clock range:  12.00 to 400.00 MHz
(II) NV(0): Not using default mode "640x350" (vrefresh out of range)
(II) NV(0): Not using default mode "320x175" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "640x400" (vrefresh out of range)
(II) NV(0): Not using default mode "320x200" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "720x400" (vrefresh out of range)
(II) NV(0): Not using default mode "360x200" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "320x240" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "640x480" (vrefresh out of range)
(II) NV(0): Not using default mode "320x240" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "640x480" (vrefresh out of range)
(II) NV(0): Not using default mode "320x240" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "640x480" (hsync out of range)
(II) NV(0): Not using default mode "320x240" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "400x300" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "400x300" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "800x600" (hsync out of range)
(II) NV(0): Not using default mode "400x300" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "800x600" (hsync out of range)
(II) NV(0): Not using default mode "400x300" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "800x600" (hsync out of range)
(II) NV(0): Not using default mode "400x300" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1024x768" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "512x384" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1024x768" (hsync out of range)
(II) NV(0): Not using default mode "512x384" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1024x768" (hsync out of range)
(II) NV(0): Not using default mode "512x384" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1024x768" (hsync out of range)
(II) NV(0): Not using default mode "512x384" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1024x768" (hsync out of range)
(II) NV(0): Not using default mode "512x384" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1152x864" (exceeds panel dimensions)
(II) NV(0): Not using default mode "576x432" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1280x960" (exceeds panel dimensions)
(II) NV(0): Not using default mode "640x480" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1280x960" (exceeds panel dimensions)
(II) NV(0): Not using default mode "640x480" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1280x1024" (exceeds panel dimensions)
(II) NV(0): Not using default mode "640x512" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1280x1024" (exceeds panel dimensions)
(II) NV(0): Not using default mode "640x512" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1280x1024" (exceeds panel dimensions)
(II) NV(0): Not using default mode "640x512" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1600x1200" (exceeds panel dimensions)
(II) NV(0): Not using default mode "800x600" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1600x1200" (exceeds panel dimensions)
(II) NV(0): Not using default mode "800x600" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1600x1200" (exceeds panel dimensions)
(II) NV(0): Not using default mode "800x600" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1600x1200" (exceeds panel dimensions)
(II) NV(0): Not using default mode "800x600" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1600x1200" (exceeds panel dimensions)
(II) NV(0): Not using default mode "800x600" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1792x1344" (exceeds panel dimensions)
(II) NV(0): Not using default mode "896x672" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1792x1344" (exceeds panel dimensions)
(II) NV(0): Not using default mode "896x672" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1856x1392" (exceeds panel dimensions)
(II) NV(0): Not using default mode "928x696" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1856x1392" (exceeds panel dimensions)
(II) NV(0): Not using default mode "928x696" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1920x1440" (exceeds panel dimensions)
(II) NV(0): Not using default mode "960x720" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1920x1440" (exceeds panel dimensions)
(II) NV(0): Not using default mode "960x720" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "832x624" (hsync out of range)
(II) NV(0): Not using default mode "416x312" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1152x768" (exceeds panel dimensions)
(II) NV(0): Not using default mode "576x384" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1400x1050" (exceeds panel dimensions)
(II) NV(0): Not using default mode "700x525" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1400x1050" (exceeds panel dimensions)
(II) NV(0): Not using default mode "700x525" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1600x1024" (exceeds panel dimensions)
(II) NV(0): Not using default mode "800x512" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "1920x1440" (exceeds panel dimensions)
(II) NV(0): Not using default mode "960x720" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "2048x1536" (exceeds panel dimensions)
(II) NV(0): Not using default mode "1024x768" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "2048x1536" (exceeds panel dimensions)
(II) NV(0): Not using default mode "1024x768" (bad mode clock/interlace/doublescan)
(II) NV(0): Not using default mode "2048x1536" (exceeds panel dimensions)
(II) NV(0): Not using default mode "1024x768" (bad mode clock/interlace/doublescan)
(--) NV(0): Virtual size is 800x600 (pitch 800)
(**) NV(0): *Default mode "800x600": 40.0 MHz, 37.9 kHz, 60.3 Hz
(II) NV(0): Modeline "800x600"   40.00  800 840 968 1056  600 601 605 628 +hsync +vsync
(**) NV(0): *Default mode "640x480": 25.2 MHz, 31.5 kHz, 59.9 Hz
(II) NV(0): Modeline "640x480"   25.18  640 656 752 800  480 490 492 525 -hsync -vsync
(**) NV(0):  Default mode "800x600": 36.0 MHz, 35.2 kHz, 56.2 Hz
(II) NV(0): Modeline "800x600"   36.00  800 824 896 1024  600 601 603 625 +hsync +vsync
(++) NV(0): DPI set to (80, 80)
(II) Loading sub module "fb"
(II) LoadModule: "fb"
(II) Loading /usr/lib64/X11/modules//libfb.so
(II) Module fb: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	ABI class: X.Org ANSI C Emulation, version 0.3
(II) Loading sub module "xaa"
(II) LoadModule: "xaa"
(II) Loading /usr/lib64/X11/modules//libxaa.so
(II) Module xaa: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.2.0
	ABI class: X.Org Video Driver, version 1.1
(II) Loading sub module "ramdac"
(II) LoadModule: "ramdac"
(II) Loading /usr/lib64/X11/modules//libramdac.so
(II) Module ramdac: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 0.1.0
	ABI class: X.Org Video Driver, version 1.1
(--) Depth 24 pixmap format is 32 bpp
(II) do I need RAC?  No, I don't.
(II) resource ranges after preInit:
	[0] 0	0	0xfc000000 - 0xfcffffff (0x1000000) MX[B]
	[1] 0	0	0xd0000000 - 0xdfffffff (0x10000000) MX[B]
	[2] 0	0	0xfb000000 - 0xfbffffff (0x1000000) MX[B]
	[3] -1	0	0x00100000 - 0x3fffffff (0x3ff00000) MX[B]E(B)
	[4] -1	0	0x000f0000 - 0x000fffff (0x10000) MX[B]
	[5] -1	0	0x000c0000 - 0x000effff (0x30000) MX[B]
	[6] -1	0	0x00000000 - 0x0009ffff (0xa0000) MX[B]
	[7] -1	0	0xfdbf8000 - 0xfdbfbfff (0x4000) MX[B]
	[8] -1	0	0xfdbff000 - 0xfdbff7ff (0x800) MX[B]
	[9] -1	0	0xfe02c000 - 0xfe02cfff (0x1000) MX[B]
	[10] -1	0	0xfe028000 - 0xfe02bfff (0x4000) MX[B]
	[11] -1	0	0xfe02d000 - 0xfe02dfff (0x1000) MX[B]
	[12] -1	0	0xfe02e000 - 0xfe02e0ff (0x100) MX[B]
	[13] -1	0	0xfe02f000 - 0xfe02ffff (0x1000) MX[B]
	[14] -1	0	0xfc000000 - 0xfcffffff (0x1000000) MX[B](B)
	[15] -1	0	0xd0000000 - 0xdfffffff (0x10000000) MX[B](B)
	[16] -1	0	0xfb000000 - 0xfbffffff (0x1000000) MX[B](B)
	[17] 0	0	0x000a0000 - 0x000affff (0x10000) MS[B](OprD)
	[18] 0	0	0x000b0000 - 0x000b7fff (0x8000) MS[B](OprD)
	[19] 0	0	0x000b8000 - 0x000bffff (0x8000) MS[B](OprD)
	[20] -1	0	0x0000ffff - 0x0000ffff (0x1) IX[B]
	[21] -1	0	0x00000000 - 0x000000ff (0x100) IX[B]
	[22] -1	0	0x0000a800 - 0x0000a80f (0x10) IX[B]
	[23] -1	0	0x0000ac00 - 0x0000ac7f (0x80) IX[B]
	[24] -1	0	0x0000dc00 - 0x0000dc07 (0x8) IX[B]
	[25] -1	0	0x0000e000 - 0x0000e00f (0x10) IX[B]
	[26] -1	0	0x00000b70 - 0x00000b73 (0x4) IX[B]
	[27] -1	0	0x00000970 - 0x00000977 (0x8) IX[B]
	[28] -1	0	0x00000bf0 - 0x00000bf3 (0x4) IX[B]
	[29] -1	0	0x000009f0 - 0x000009f7 (0x8) IX[B]
	[30] -1	0	0x0000f400 - 0x0000f40f (0x10) IX[B]
	[31] -1	0	0x00004c40 - 0x00004c7f (0x40) IX[B]
	[32] -1	0	0x00004c00 - 0x00004c3f (0x40) IX[B]
	[33] 0	0	0x000003b0 - 0x000003bb (0xc) IS[B](OprU)
	[34] 0	0	0x000003c0 - 0x000003df (0x20) IS[B](OprU)
(==) NV(0): Write-combining range (0xd0000000,0x2000000)
(II) NV(0): Using XFree86 Acceleration Architecture (XAA)
	Screen to screen bit blits
	Solid filled rectangles
	8x8 mono pattern filled rectangles
	Indirect CPU to Screen color expansion
	Solid Lines
	Scanline Image Writes
	Offscreen Pixmaps
	Setting up tile and stipple cache:
		32 128x128 slots
		32 256x256 slots
		16 512x512 slots
(==) NV(0): Backing store disabled
(==) NV(0): Silken mouse enabled
(==) RandR enabled
(II) Initializing built-in extension MIT-SHM
(II) Initializing built-in extension XInputExtension
(II) Initializing built-in extension XTEST
(II) Initializing built-in extension XKEYBOARD
(II) Initializing built-in extension XC-APPGROUP
(II) Initializing built-in extension XAccessControlExtension
(II) Initializing built-in extension SECURITY
(II) Initializing built-in extension XINERAMA
(II) Initializing built-in extension XFIXES
(II) Initializing built-in extension XFree86-Bigfont
(II) Initializing built-in extension RENDER
(II) Initializing built-in extension RANDR
(II) Initializing built-in extension COMPOSITE
(II) Initializing built-in extension DAMAGE
(II) Initializing built-in extension XEVIE
(II) Loading local sub module "GLcore"
(II) LoadModule: "GLcore"
(II) Loading /usr/lib64/X11/modules/extensions//libGLcore.so
(II) Module GLcore: vendor="X.Org Foundation"
	compiled for 7.2.0, module version = 1.0.0
	ABI class: X.Org Server Extension, version 0.3
(II) GLX: Initialized MESA-PROXY GL provider for screen 0
(**) Option "Protocol" "auto"
(**) Mouse0: Device: "/dev/input/mice"
(**) Mouse0: Protocol: "auto"
(**) Option "CorePointer"
(**) Mouse0: Core Pointer
(**) Option "Device" "/dev/input/mice"
(==) Mouse0: Emulate3Buttons, Emulate3Timeout: 50
(**) Mouse0: ZAxisMapping: buttons 4 and 5
(**) Mouse0: Buttons: 9
(**) Option "CoreKeyboard"
(**) Keyboard0: Core Keyboard
(**) Option "Protocol" "standard"
(**) Keyboard0: Protocol: standard
(**) Option "AutoRepeat" "500 30"
(**) Option "XkbRules" "xorg"
(**) Keyboard0: XkbRules: "xorg"
(**) Option "XkbModel" "pc105"
(**) Keyboard0: XkbModel: "pc105"
(**) Option "XkbLayout" "us"
(**) Keyboard0: XkbLayout: "us"
(**) Option "CustomKeycodes" "off"
(**) Keyboard0: CustomKeycodes disabled
(II) XINPUT: Adding extended input device "Keyboard0" (type: KEYBOARD)
(II) XINPUT: Adding extended input device "Mouse0" (type: MOUSE)
(--) Mouse0: PnP-detected protocol: "ExplorerPS/2"
(II) Mouse0: ps2EnableDataReporting: succeeded
(II) Mouse0: ps2EnableDataReporting: succeeded
(II) Mouse0: ps2EnableDataReporting: succeeded
(II) Mouse0: ps2EnableDataReporting: succeeded
